ISO Thread Specifications

Metric threads only.

M 16 x 2 - 4h -5H

M --- ISO Metric designation

16 --- Nominal diameter in millimeters

2 --- Thread pitch in millimeters (distance from top of one thread to top of the next)

4h --- Class of fit of this thread (optional)

5H --- Class of fit of mating thread (optional)